WindClock-III

A full description of how to make and install your own WindClock-III will be provided here in time.

Current prototype development state:

installed a raspberry pi 3 with a sensehat again, after messing up with python 3.5

python coded all data for realtime request available in a file

managed to install a couple of working online transfers with the new websockets/html5 protocols (finalizing is and now testing websocketd which is promising easier connectivity)

Future work:

adding a waterproof temperature and ambient light sensor by extending the sensehat header pins

power: 5V-2A for the pi seems too much, so would use a Teensy with 3.3V 500mA (windclock-iv)

designing a shape/case for hanging it up and responsive to wind (physical calibration)

simple visualisation/sonification on the object (python will do, maybe puredata too)

work with more than one windclock (but keep it under 10 haha)

client-side for data capture (katastrof interpretation and sonification) in various programs

Make and install the real objects

rodchenko examples (see below)

gtr-lahaag'z ultimate design: in the atkn wiki

I would just cut out a spiral out of a thin wooden plate and stretch from the middle up

gert's suggestions for design

More details and progress the coming weeks...